Convolution and Deconvolution

Open Table or Figure or Fit Plot with initial data and select Processing → Convolution or Deconvolution menu item.

Parameters

Linear/Circular checkbox specify the signal to be treated as periodic or not.